#MicroXplorer Configuration settings - do not modify
Dma.LPUART_RX.0.Direction=DMA_PERIPH_TO_MEMORY
Dma.LPUART_RX.0.Instance=DMA2_Channel7
Dma.LPUART_RX.0.MemDataAlignment=DMA_MDATAALIGN_BYTE
Dma.LPUART_RX.0.MemInc=DMA_MINC_ENABLE
Dma.LPUART_RX.0.Mode=DMA_NORMAL
Dma.LPUART_RX.0.PeriphDataAlignment=DMA_PDATAALIGN_BYTE
Dma.LPUART_RX.0.PeriphInc=DMA_PINC_DISABLE
Dma.LPUART_RX.0.Priority=DMA_PRIORITY_LOW
Dma.LPUART_RX.0.RequestParameters=Instance,Direction,PeriphInc,MemInc,PeriphDataAlignment,MemDataAlignment,Mode,Priority
Dma.Request0=LPUART_RX
Dma.RequestsNb=1
FREERTOS.BinarySemaphores01=si5351,Dynamic,NULL;command,Dynamic,NULL
FREERTOS.FootprintOK=true
FREERTOS.IPParameters=Tasks01,configUSE_NEWLIB_REENTRANT,FootprintOK,configTOTAL_HEAP_SIZE,BinarySemaphores01,configENABLE_BACKWARD_COMPATIBILITY,configUSE_POSIX_ERRNO
FREERTOS.Tasks01=timeTask,24,128,start_time_task,Default,NULL,Dynamic,NULL,NULL;terminalTask,24,256,start_terminal_task,Default,NULL,Dynamic,NULL,NULL;morseTask,24,128,start_morse_task,Default,si5351_inst,Dynamic,NULL,NULL;clk2Task,40,128,start_clk2_task,Default,si5351_inst,Dynamic,NULL,NULL
FREERTOS.configENABLE_BACKWARD_COMPATIBILITY=0
FREERTOS.configTOTAL_HEAP_SIZE=50000
FREERTOS.configUSE_NEWLIB_REENTRANT=1
FREERTOS.configUSE_POSIX_ERRNO=0
File.Version=6
GPIO.groupedBy=Group By Peripherals
I2C1.I2C_Fall_Time=10
I2C1.I2C_Rise_Time=10
I2C1.I2C_Speed_Mode=I2C_Fast
I2C1.IPParameters=Timing,I2C_Speed_Mode,I2C_Rise_Time,I2C_Fall_Time
I2C1.Timing=0x00000001
KeepUserPlacement=false
LPUART1.AutoBaudRateEnableParam=UART_ADVFEATURE_AUTOBAUDRATE_DISABLE
LPUART1.BaudRate=115200
LPUART1.DMADisableonRxErrorParam=UART_ADVFEATURE_DMA_DISABLEONRXERROR
LPUART1.DataInvertParam=UART_ADVFEATURE_DATAINV_DISABLE
LPUART1.IPParameters=WordLength,Parity,StopBits,Mode,OneBitSampling,AutoBaudRateEnableParam,TxPinLevelInvertParam,RxPinLevelInvertParam,DataInvertParam,SwapParam,OverrunDisableParam,DMADisableonRxErrorParam,MSBFirstParam,BaudRate
LPUART1.MSBFirstParam=UART_ADVFEATURE_MSBFIRST_DISABLE
LPUART1.Mode=UART_MODE_TX_RX
LPUART1.OneBitSampling=UART_ONE_BIT_SAMPLE_DISABLE
LPUART1.OverrunDisableParam=UART_ADVFEATURE_OVERRUN_DISABLE
LPUART1.Parity=UART_PARITY_NONE
LPUART1.RxPinLevelInvertParam=UART_ADVFEATURE_RXINV_DISABLE
LPUART1.StopBits=UART_STOPBITS_1
LPUART1.SwapParam=UART_ADVFEATURE_SWAP_DISABLE
LPUART1.TxPinLevelInvertParam=UART_ADVFEATURE_TXINV_DISABLE
LPUART1.WordLength=UART_WORDLENGTH_8B
Mcu.CPN=STM32L4A6ZGT6
Mcu.Family=STM32L4
Mcu.IP0=DMA
Mcu.IP1=FREERTOS
Mcu.IP2=I2C1
Mcu.IP3=LPUART1
Mcu.IP4=NVIC
Mcu.IP5=RCC
Mcu.IP6=RTC
Mcu.IP7=SYS
Mcu.IPNb=8
Mcu.Name=STM32L4A6ZGTx
Mcu.Package=LQFP144
Mcu.Pin0=PE2
Mcu.Pin1=PE3
Mcu.Pin10=PF2
Mcu.Pin100=PB3 (JTDO/TRACESWO)
Mcu.Pin101=PB4 (NJTRST)
Mcu.Pin102=PB5
Mcu.Pin103=PB6
Mcu.Pin104=PB7
Mcu.Pin105=PH3-BOOT0
Mcu.Pin106=PB8
Mcu.Pin107=PB9
Mcu.Pin108=VP_FREERTOS_VS_CMSIS_V2
Mcu.Pin109=VP_RTC_VS_RTC_Activate
Mcu.Pin11=PF3
Mcu.Pin110=VP_RTC_VS_RTC_Calendar
Mcu.Pin111=VP_SYS_VS_tim6
Mcu.Pin12=PF4
Mcu.Pin13=PF5
Mcu.Pin14=PF6
Mcu.Pin15=PF7
Mcu.Pin16=PF8
Mcu.Pin17=PF9
Mcu.Pin18=PF10
Mcu.Pin19=PH0-OSC_IN (PH0)
Mcu.Pin2=PE4
Mcu.Pin20=PH1-OSC_OUT (PH1)
Mcu.Pin21=PC0
Mcu.Pin22=PC1
Mcu.Pin23=PC2
Mcu.Pin24=PC3
Mcu.Pin25=PA0
Mcu.Pin26=PA1
Mcu.Pin27=PA2
Mcu.Pin28=PA3
Mcu.Pin29=PA4
Mcu.Pin3=PE5
Mcu.Pin30=PA5
Mcu.Pin31=PA6
Mcu.Pin32=PA7
Mcu.Pin33=PC4
Mcu.Pin34=PC5
Mcu.Pin35=PB0
Mcu.Pin36=PB2
Mcu.Pin37=PF11
Mcu.Pin38=PF12
Mcu.Pin39=PF13
Mcu.Pin4=PE6
Mcu.Pin40=PF14
Mcu.Pin41=PF15
Mcu.Pin42=PG0
Mcu.Pin43=PG1
Mcu.Pin44=PE7
Mcu.Pin45=PE8
Mcu.Pin46=PE9
Mcu.Pin47=PE10
Mcu.Pin48=PE11
Mcu.Pin49=PE12
Mcu.Pin5=PC13
Mcu.Pin50=PE13
Mcu.Pin51=PE14
Mcu.Pin52=PE15
Mcu.Pin53=PB10
Mcu.Pin54=PB11
Mcu.Pin55=PB12
Mcu.Pin56=PB13
Mcu.Pin57=PB14
Mcu.Pin58=PB15
Mcu.Pin59=PD8
Mcu.Pin6=PC14-OSC32_IN (PC14)
Mcu.Pin60=PD9
Mcu.Pin61=PD10
Mcu.Pin62=PD11
Mcu.Pin63=PD12
Mcu.Pin64=PD13
Mcu.Pin65=PD14
Mcu.Pin66=PD15
Mcu.Pin67=PG2
Mcu.Pin68=PG3
Mcu.Pin69=PG4
Mcu.Pin7=PC15-OSC32_OUT (PC15)
Mcu.Pin70=PG5
Mcu.Pin71=PG6
Mcu.Pin72=PG7
Mcu.Pin73=PG8
Mcu.Pin74=PC6
Mcu.Pin75=PC7
Mcu.Pin76=PC8
Mcu.Pin77=PC9
Mcu.Pin78=PA8
Mcu.Pin79=PA9
Mcu.Pin8=PF0
Mcu.Pin80=PA10
Mcu.Pin81=PA11
Mcu.Pin82=PA12
Mcu.Pin83=PA13 (JTMS/SWDIO)
Mcu.Pin84=PA14 (JTCK/SWCLK)
Mcu.Pin85=PA15 (JTDI)
Mcu.Pin86=PD0
Mcu.Pin87=PD1
Mcu.Pin88=PD3
Mcu.Pin89=PD4
Mcu.Pin9=PF1
Mcu.Pin90=PD5
Mcu.Pin91=PD6
Mcu.Pin92=PD7
Mcu.Pin93=PG9
Mcu.Pin94=PG10
Mcu.Pin95=PG11
Mcu.Pin96=PG12
Mcu.Pin97=PG13
Mcu.Pin98=PG14
Mcu.Pin99=PG15
Mcu.PinsNb=112
Mcu.ThirdPartyNb=0
Mcu.UserConstants=
Mcu.UserName=STM32L4A6ZGTx
MxCube.Version=6.6.1
MxDb.Version=DB.6.0.60
NVIC.BusFault_IRQn=true\:0\:0\:false\:false\:true\:false\:true\:false\:false
NVIC.DMA2_Channel7_IRQn=true\:5\:0\:false\:false\:true\:true\:false\:true\:true
NVIC.DebugMonitor_IRQn=true\:0\:0\:false\:false\:true\:false\:true\:false\:false
NVIC.ForceEnableDMAVector=true
NVIC.HardFault_IRQn=true\:0\:0\:false\:false\:true\:false\:true\:false\:false
NVIC.LPUART1_IRQn=true\:5\:0\:false\:false\:true\:true\:true\:true\:true
NVIC.MemoryManagement_IRQn=true\:0\:0\:false\:false\:true\:false\:true\:false\:false
NVIC.NonMaskableInt_IRQn=true\:0\:0\:false\:false\:true\:false\:true\:false\:false
NVIC.PendSV_IRQn=true\:15\:0\:false\:false\:false\:true\:true\:false\:false
NVIC.PriorityGroup=NVIC_PRIORITYGROUP_4
NVIC.SVCall_IRQn=true\:0\:0\:false\:false\:false\:false\:true\:false\:false
NVIC.SavedPendsvIrqHandlerGenerated=true
NVIC.SavedSvcallIrqHandlerGenerated=true
NVIC.SavedSystickIrqHandlerGenerated=true
NVIC.SysTick_IRQn=true\:15\:0\:false\:false\:false\:true\:true\:true\:false
NVIC.TIM6_DAC_IRQn=true\:15\:0\:false\:false\:true\:false\:false\:true\:true
NVIC.TimeBase=TIM6_DAC_IRQn
NVIC.TimeBaseIP=TIM6
NVIC.UsageFault_IRQn=true\:0\:0\:false\:false\:true\:false\:true\:false\:false
PA0.Signal=GPIO_Analog
PA1.Signal=GPIO_Analog
PA10.GPIOParameters=GPIO_Label
PA10.GPIO_Label=USB_ID
PA10.Locked=true
PA10.Signal=USB_OTG_FS_ID
PA11.GPIOParameters=GPIO_Label
PA11.GPIO_Label=USB_DM
PA11.Locked=true
PA11.Signal=USB_OTG_FS_DM
PA12.GPIOParameters=GPIO_Label
PA12.GPIO_Label=USB_DP
PA12.Locked=true
PA12.Signal=USB_OTG_FS_DP
PA13\ (JTMS/SWDIO).GPIOParameters=GPIO_Label
PA13\ (JTMS/SWDIO).GPIO_Label=TMS
PA13\ (JTMS/SWDIO).Locked=true
PA13\ (JTMS/SWDIO).Mode=Trace_Asynchronous_SW
PA13\ (JTMS/SWDIO).Signal=SYS_JTMS-SWDIO
PA14\ (JTCK/SWCLK).GPIOParameters=GPIO_Label
PA14\ (JTCK/SWCLK).GPIO_Label=TCK
PA14\ (JTCK/SWCLK).Locked=true
PA14\ (JTCK/SWCLK).Mode=Trace_Asynchronous_SW
PA14\ (JTCK/SWCLK).Signal=SYS_JTCK-SWCLK
PA15\ (JTDI).Signal=GPIO_Analog
PA2.Mode=Clock-out-LSCO
PA2.Signal=RCC_LSCO
PA3.Signal=GPIO_Analog
PA4.Signal=GPIO_Analog
PA5.Signal=GPIO_Analog
PA6.Signal=GPIO_Analog
PA7.Signal=GPIO_Analog
PA8.GPIOParameters=GPIO_Label
PA8.GPIO_Label=USB_SOF [TP1]
PA8.Locked=true
PA8.Signal=USB_OTG_FS_SOF
PA9.GPIOParameters=GPIO_Label
PA9.GPIO_Label=USB_VBUS
PA9.Locked=true
PA9.Signal=USB_OTG_FS_VBUS
PB0.Signal=GPIO_Analog
PB10.Signal=GPIO_Analog
PB11.Signal=GPIO_Analog
PB12.Signal=GPIO_Analog
PB13.Signal=GPIO_Analog
PB14.GPIOParameters=GPIO_Label
PB14.GPIO_Label=LD3 [Red]
PB14.Locked=true
PB14.Signal=GPIO_Output
PB15.Signal=GPIO_Analog
PB2.Signal=GPIO_Analog
PB3\ (JTDO/TRACESWO).GPIOParameters=GPIO_Label
PB3\ (JTDO/TRACESWO).GPIO_Label=SWO
PB3\ (JTDO/TRACESWO).Locked=true
PB3\ (JTDO/TRACESWO).Mode=Trace_Asynchronous_SW
PB3\ (JTDO/TRACESWO).Signal=SYS_JTDO-SWO
PB4\ (NJTRST).Signal=GPIO_Analog
PB5.Signal=GPIO_Analog
PB6.Signal=GPIO_Analog
PB7.GPIOParameters=GPIO_Label
PB7.GPIO_Label=LD2 [Blue]
PB7.Locked=true
PB7.Signal=GPIO_Output
PB8.GPIOParameters=GPIO_Pu
PB8.GPIO_Pu=GPIO_PULLUP
PB8.Locked=true
PB8.Mode=I2C
PB8.Signal=I2C1_SCL
PB9.GPIOParameters=GPIO_Pu
PB9.GPIO_Pu=GPIO_PULLUP
PB9.Locked=true
PB9.Mode=I2C
PB9.Signal=I2C1_SDA
PC0.Signal=GPIO_Analog
PC1.Signal=GPIO_Analog
PC13.GPIOParameters=GPIO_PuPd,GPIO_Label
PC13.GPIO_Label=B1
PC13.GPIO_PuPd=GPIO_PULLDOWN
PC13.Locked=true
PC13.Signal=GPIO_Input
PC14-OSC32_IN\ (PC14).Locked=true
PC14-OSC32_IN\ (PC14).Mode=LSE-External-Oscillator
PC14-OSC32_IN\ (PC14).Signal=RCC_OSC32_IN
PC15-OSC32_OUT\ (PC15).Locked=true
PC15-OSC32_OUT\ (PC15).Mode=LSE-External-Oscillator
PC15-OSC32_OUT\ (PC15).Signal=RCC_OSC32_OUT
PC2.Signal=GPIO_Analog
PC3.Signal=GPIO_Analog
PC4.Signal=GPIO_Analog
PC5.Signal=GPIO_Analog
PC6.Signal=GPIO_Analog
PC7.GPIOParameters=GPIO_Label
PC7.GPIO_Label=LD1 [Green]
PC7.Locked=true
PC7.Signal=GPIO_Output
PC8.Signal=GPIO_Analog
PC9.Signal=GPIO_Analog
PCC.Checker=true
PCC.Line=STM32L4x6
PCC.MCU=STM32L4A6ZGTx
PCC.PartNumber=STM32L4A6ZGTx
PCC.Seq0=2
PCC.Seq0.Step0.Average_Current=2.12 mA
PCC.Seq0.Step0.CPU_Frequency=16 MHz
PCC.Seq0.Step0.Category=In DS Table
PCC.Seq0.Step0.DMIPS=20.0
PCC.Seq0.Step0.Duration=0.1 ms
PCC.Seq0.Step0.Frequency=16 MHz
PCC.Seq0.Step0.Memory=SRAM2
PCC.Seq0.Step0.Mode=RUN
PCC.Seq0.Step0.Oscillator=HSE BYP Flash-PowerDown
PCC.Seq0.Step0.Peripherals=
PCC.Seq0.Step0.TaMax=104.8
PCC.Seq0.Step0.User's_Consumption=0 mA
PCC.Seq0.Step0.Vcore=Range1-High
PCC.Seq0.Step0.Vdd=3.0
PCC.Seq0.Step0.Voltage_Source=Battery
PCC.Seq0.Step1.Average_Current=131 \u00B5A
PCC.Seq0.Step1.CPU_Frequency=32.768 kHz
PCC.Seq0.Step1.Category=In DS Table
PCC.Seq0.Step1.DMIPS=0.0
PCC.Seq0.Step1.Duration=0.9 ms
PCC.Seq0.Step1.Frequency=32.768 kHz
PCC.Seq0.Step1.Memory=n/a
PCC.Seq0.Step1.Mode=STOP0
PCC.Seq0.Step1.Oscillator=LSE BYP Flash-PowerDown
PCC.Seq0.Step1.Peripherals=
PCC.Seq0.Step1.TaMax=104.99
PCC.Seq0.Step1.User's_Consumption=0 mA
PCC.Seq0.Step1.Vcore=NoRange
PCC.Seq0.Step1.Vdd=3.0
PCC.Seq0.Step1.Voltage_Source=Battery
PCC.Series=STM32L4
PCC.Temperature=25
PCC.Vdd=3.0
PD0.Signal=GPIO_Analog
PD1.Signal=GPIO_Analog
PD10.Signal=GPIO_Analog
PD11.Signal=GPIO_Analog
PD12.Signal=GPIO_Analog
PD13.Signal=GPIO_Analog
PD14.Signal=GPIO_Analog
PD15.Signal=GPIO_Analog
PD3.Signal=GPIO_Analog
PD4.Signal=GPIO_Analog
PD5.Signal=GPIO_Analog
PD6.Signal=GPIO_Analog
PD7.Signal=GPIO_Analog
PD8.Signal=GPIO_Analog
PD9.Signal=GPIO_Analog
PE10.Signal=GPIO_Analog
PE11.Signal=GPIO_Analog
PE12.Signal=GPIO_Analog
PE13.Signal=GPIO_Analog
PE14.Signal=GPIO_Analog
PE15.Signal=GPIO_Analog
PE2.Signal=GPIO_Analog
PE3.Signal=GPIO_Analog
PE4.Signal=GPIO_Analog
PE5.Signal=GPIO_Analog
PE6.Signal=GPIO_Analog
PE7.Signal=GPIO_Analog
PE8.Signal=GPIO_Analog
PE9.Signal=GPIO_Analog
PF0.Signal=GPIO_Analog
PF1.Signal=GPIO_Analog
PF10.Signal=GPIO_Analog
PF11.Signal=GPIO_Analog
PF12.Signal=GPIO_Analog
PF13.Signal=GPIO_Analog
PF14.Signal=GPIO_Analog
PF15.Signal=GPIO_Analog
PF2.Signal=GPIO_Analog
PF3.Signal=GPIO_Analog
PF4.Signal=GPIO_Analog
PF5.Signal=GPIO_Analog
PF6.Signal=GPIO_Analog
PF7.Signal=GPIO_Analog
PF8.Signal=GPIO_Analog
PF9.Signal=GPIO_Analog
PG0.Signal=GPIO_Analog
PG1.Signal=GPIO_Analog
PG10.Signal=GPIO_Analog
PG11.Signal=GPIO_Analog
PG12.Signal=GPIO_Analog
PG13.Signal=GPIO_Analog
PG14.Signal=GPIO_Analog
PG15.Signal=GPIO_Analog
PG2.Signal=GPIO_Analog
PG3.Signal=GPIO_Analog
PG4.Signal=GPIO_Analog
PG5.GPIOParameters=GPIO_Label
PG5.GPIO_Label=USB_OverCurrent [STMPS2151STR_FAULT]
PG5.Locked=true
PG5.Signal=GPIO_Input
PG6.Locked=true
PG6.Signal=GPIO_Output
PG7.GPIOParameters=GPIO_Speed,GPIO_Label
PG7.GPIO_Label=STLK_RX [STM32F103CBT6_PA3]
PG7.GPIO_Speed=GPIO_SPEED_FREQ_HIGH
PG7.Locked=true
PG7.Mode=Asynchronous
PG7.Signal=LPUART1_TX
PG8.GPIOParameters=GPIO_Speed,GPIO_Label
PG8.GPIO_Label=STLK_TX [STM32F103CBT6_PA2]
PG8.GPIO_Speed=GPIO_SPEED_FREQ_HIGH
PG8.Locked=true
PG8.Mode=Asynchronous
PG8.Signal=LPUART1_RX
PG9.Signal=GPIO_Analog
PH0-OSC_IN\ (PH0).Signal=GPIO_Analog
PH1-OSC_OUT\ (PH1).Locked=true
PH1-OSC_OUT\ (PH1).Signal=RCC_OSC_OUT
PH3-BOOT0.Signal=GPIO_Analog
PinOutPanel.RotationAngle=0
ProjectManager.AskForMigrate=true
ProjectManager.BackupPrevious=false
ProjectManager.CompilerOptimize=6
ProjectManager.ComputerToolchain=false
ProjectManager.CoupleFile=false
ProjectManager.CustomerFirmwarePackage=
ProjectManager.DefaultFWLocation=true
ProjectManager.DeletePrevious=true
ProjectManager.DeviceId=STM32L4A6ZGTx
ProjectManager.FirmwarePackage=STM32Cube FW_L4 V1.17.2
ProjectManager.FreePins=true
ProjectManager.HalAssertFull=false
ProjectManager.HeapSize=0x200
ProjectManager.KeepUserCode=true
ProjectManager.LastFirmware=true
ProjectManager.LibraryCopy=1
ProjectManager.MainLocation=Core/Src
ProjectManager.NoMain=false
ProjectManager.PreviousToolchain=
ProjectManager.ProjectBuild=false
ProjectManager.ProjectFileName=stm32l4a6zg-f0x.at1.ioc
ProjectManager.ProjectName=stm32l4a6zg-f0x.at1
ProjectManager.RegisterCallBack=
ProjectManager.StackSize=0x400
ProjectManager.TargetToolchain=STM32CubeIDE
ProjectManager.ToolChainLocation=
ProjectManager.UnderRoot=true
ProjectManager.functionlistsort=1-SystemClock_Config-RCC-false-HAL-false,2-MX_GPIO_Init-GPIO-false-HAL-true,3-MX_DMA_Init-DMA-false-HAL-true,4-MX_I2C1_Init-I2C1-false-HAL-true,5-MX_LPUART1_UART_Init-LPUART1-false-HAL-true,6-MX_RTC_Init-RTC-false-HAL-true
RCC.ADCFreq_Value=48000000
RCC.AHBCLKDivider=RCC_SYSCLK_DIV8
RCC.AHBFreq_Value=5916666.666666667
RCC.APB1CLKDivider=RCC_HCLK_DIV2
RCC.APB1Freq_Value=2958333.3333333335
RCC.APB1TimFreq_Value=5916666.666666667
RCC.APB2CLKDivider=RCC_HCLK_DIV4
RCC.APB2Freq_Value=1479166.6666666667
RCC.APB2TimFreq_Value=2958333.3333333335
RCC.CortexFreq_Value=5916666.666666667
RCC.DFSDMFreq_Value=2958333.3333333335
RCC.FCLKCortexFreq_Value=5916666.666666667
RCC.FamilyName=M
RCC.HCLKFreq_Value=5916666.666666667
RCC.HSE_VALUE=8000000
RCC.HSI48_VALUE=48000000
RCC.HSI_VALUE=16000000
RCC.I2C1Freq_Value=2958333.3333333335
RCC.I2C2Freq_Value=2958333.3333333335
RCC.I2C3Freq_Value=2958333.3333333335
RCC.I2C4Freq_Value=2958333.3333333335
RCC.IPParameters=ADCFreq_Value,AHBCLKDivider,AHBFreq_Value,APB1CLKDivider,APB1Freq_Value,APB1TimFreq_Value,APB2CLKDivider,APB2Freq_Value,APB2TimFreq_Value,CortexFreq_Value,DFSDMFreq_Value,FCLKCortexFreq_Value,FamilyName,HCLKFreq_Value,HSE_VALUE,HSI48_VALUE,HSI_VALUE,I2C1Freq_Value,I2C2Freq_Value,I2C3Freq_Value,I2C4Freq_Value,LCDFreq_Value,LPTIM1Freq_Value,LPTIM2Freq_Value,LPUART1Freq_Value,LSCOPinFreq_Value,LSI_VALUE,MCO1PinFreq_Value,MSI_VALUE,PLLN,PLLPoutputFreq_Value,PLLQoutputFreq_Value,PLLR,PLLRCLKFreq_Value,PLLSAI1N,PLLSAI1PoutputFreq_Value,PLLSAI1QoutputFreq_Value,PLLSAI1RoutputFreq_Value,PLLSAI2PoutputFreq_Value,PLLSAI2RoutputFreq_Value,PWRFreq_Value,RNGFreq_Value,RTCClockSelection,RTCFreq_Value,SAI1Freq_Value,SAI2Freq_Value,SDMMCFreq_Value,SWPMI1Freq_Value,SYSCLKFreq_VALUE,SYSCLKSource,UART4Freq_Value,UART5Freq_Value,USART1Freq_Value,USART2Freq_Value,USART3Freq_Value,USBFreq_Value,VCOInputFreq_Value,VCOOutputFreq_Value,VCOSAI1OutputFreq_Value,VCOSAI2OutputFreq_Value
RCC.LCDFreq_Value=32768
RCC.LPTIM1Freq_Value=2958333.3333333335
RCC.LPTIM2Freq_Value=2958333.3333333335
RCC.LPUART1Freq_Value=2958333.3333333335
RCC.LSCOPinFreq_Value=32000
RCC.LSI_VALUE=32000
RCC.MCO1PinFreq_Value=47333333.333333336
RCC.MSI_VALUE=4000000
RCC.PLLN=71
RCC.PLLPoutputFreq_Value=142000000
RCC.PLLQoutputFreq_Value=142000000
RCC.PLLR=RCC_PLLR_DIV6
RCC.PLLRCLKFreq_Value=47333333.333333336
RCC.PLLSAI1N=24
RCC.PLLSAI1PoutputFreq_Value=48000000
RCC.PLLSAI1QoutputFreq_Value=48000000
RCC.PLLSAI1RoutputFreq_Value=48000000
RCC.PLLSAI2PoutputFreq_Value=16000000
RCC.PLLSAI2RoutputFreq_Value=16000000
RCC.PWRFreq_Value=47333333.333333336
RCC.RNGFreq_Value=48000000
RCC.RTCClockSelection=RCC_RTCCLKSOURCE_LSE
RCC.RTCFreq_Value=32768
RCC.SAI1Freq_Value=48000000
RCC.SAI2Freq_Value=48000000
RCC.SDMMCFreq_Value=48000000
RCC.SWPMI1Freq_Value=2958333.3333333335
RCC.SYSCLKFreq_VALUE=47333333.333333336
RCC.SYSCLKSource=RCC_SYSCLKSOURCE_PLLCLK
RCC.UART4Freq_Value=2958333.3333333335
RCC.UART5Freq_Value=2958333.3333333335
RCC.USART1Freq_Value=1479166.6666666667
RCC.USART2Freq_Value=2958333.3333333335
RCC.USART3Freq_Value=2958333.3333333335
RCC.USBFreq_Value=48000000
RCC.VCOInputFreq_Value=4000000
RCC.VCOOutputFreq_Value=284000000
RCC.VCOSAI1OutputFreq_Value=96000000
RCC.VCOSAI2OutputFreq_Value=32000000
RTC.Date=1
RTC.Hours=0
RTC.IPParameters=Hours,Minutes,Month,Date,Year,StoreOperation
RTC.Minutes=0
RTC.Month=RTC_MONTH_AUGUST
RTC.StoreOperation=RTC_STOREOPERATION_RESET
RTC.Year=22
VP_FREERTOS_VS_CMSIS_V2.Mode=CMSIS_V2
VP_FREERTOS_VS_CMSIS_V2.Signal=FREERTOS_VS_CMSIS_V2
VP_RTC_VS_RTC_Activate.Mode=RTC_Enabled
VP_RTC_VS_RTC_Activate.Signal=RTC_VS_RTC_Activate
VP_RTC_VS_RTC_Calendar.Mode=RTC_Calendar
VP_RTC_VS_RTC_Calendar.Signal=RTC_VS_RTC_Calendar
VP_SYS_VS_tim6.Mode=TIM6
VP_SYS_VS_tim6.Signal=SYS_VS_tim6
board=NUCLEO-L4A6ZG
isbadioc=false
